# Example muster list

Abandon ship = 7 short 1 long on the ship's horn Fire = continuous ringing bell

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Muster list SL-9: In the event of an incident, the alarm is triggered by the skipper or his replacement, orally the nature of the incident is stated. | | | | |
| **Rank** | **Lifeboat muster** | **Fire muster** | **Man overboard** | **Sopep** |
| Skipper | Bridge, general management:  • maintains radio contact and navigates, takes with SART, Pyrotechnics, VHF radios and ship's diary. | Bridge, general management:  • maintains radio contact and navigates, closes the fire dampers on the bridge. | Bridge, general management:  • maintains radio contact and navigates, plots the position of the drowning person on the map, keeps an eye on the drowning person. | Bridge, general management: |
| Engineer *Replaces skipper* | • Assists in preparing the life raft. | • Starts the deck wash pump, closes the fire dampers in the winch room, stops the ventilation, closes the SOS valves if necessary, operates the fixed fire extinguishing system in the engine room. | • Maintains communication with the bridge, keeps an eye on the drowning person. | • Closes valves or stops oil transfer, directs clean-up operations. |
| Deckhand 1 *Replaces engineer or deckhand 3* | • Prepares the rafts on behalf of the skipper, brings along EPIRB. | • Prepares fire hoses, assists the engineer. | • Keeps an eye on the drowning person, assists the engineer. | • Assists the engineer in clean-up work. |
| Deckhand 2 *Replaces deckhand 1* | • Brings along survival suits and life jackets from of the cabins. Assists with preparing the rafts. | • Stops ventilation in the galley, brings along small extinguishers, assists the engineer. | • Keeps an eye on the drowning person, assists the engineer. | • Assists with the clean-up work. |
| Deckhand 3 *Replaces deckhand 2* | • Brings along extra food, water and clothing, assists with preparing the rafts. | • Brings along small fire extinguishers and assists in preparing fire hoses. | • Keeps an eye on the drowning person, assists the engineer. | • Assists with the clean-up work. |
| Passager/Student | • Follows orders. | • Follows orders. | • Follows orders. | • Follows orders. |

* Abandoning ship only takes place on the instructions of the skipper or his replacement.
* The closing of the SOS valves, the activation of the engine room extinguishing system is only done by the operator and after consultation with the skipper.